|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  | **PURCHASE ORDER** | | |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
| Po no: 23-24 Q MDT 104 | | |  |  |  | Date: 10/04/2023 | |  |
| Supplier MDT Technologies GmbH | | | |  |  | Quotation: Email | | |
| Billing Address: A1, Haritaras Siddharud Sadan, Altinho Rd | | | | | |  | |  |
|  |  | St-inez Panaji - Goa India 403001 | | |  |  | | |
| Shipping Address: 114, Gera Imperium Green, Next to | | | | | |  | |  |
|  |  | Jairam complex, Mala Panaji Goa India 403001 | | | |  |  |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **SR. NO** | **Item No.** | **Product Description** | **Qty** | **Pricing Per Unit** | **Discount** | **Amount** |
| 1 | AKD-0410V.02 | Dimming Actuator 4-fold, 4SU MDRC, 1-10V, RGBW 3 years product warranty, Country of origin DE, HS Code 85365080 Dimming Actuator 4-fold, 4SU MDRC, 1-10V, RGBW. Control device for 1-10V electronic transformers with relays. Current max. 16A, capacitive load max. 140µF. Push Button for manual operation and indicator for each channel. To control 1-10V electronic transformers (ECG). With RGBW functionality. RGB und HSV control with extensive colour functions. Offers control voltage up to 30 ECG (each channel). Voltage reversal protection. Embedded switching relays for 30 ECG/30W, 20 ECG/58W, 15 ECG/2x36W, 10 ECG/2 x58W. Adjustable switch-on behaviour. Minimum/maximum brighness value adjustable. Adjustable dimming speed. Central switching functions. 8 scenes per channel. 1Bit automatic function. 3 years warranty. | 6 | 255 | 132.6 | 795.6 |
| 2 | PVK IN | handling and shipping charge / UPS express saver IN | 1 | 141 |  | 141 |
| **TOTAL (EURO)** | | | | |  | **936.6** |

Terms and conditions apply as per norms JPT001

Kindly dispatch the material as per quotation mentioned

Strictly Door delivered as per the shipping address mentioned above.