|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  | **PURCHASE ORDER** | | |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
| Po no: 23-24 Multi Bath 321 | | |  |  |  | Date: 05/12/2023 | |  |
| Supplier Multi Bath Service | | | |  |  | Quotation: Email | | |
| Billing Address: 114, Gera Imperium Green, Next to | | | | | |  | |  |
|  |  | Jairam complex, Mala Panaji Goa 403001 | | |  |  | | |
| Shipping Address: : Flat No – C 801, Edcon Rio Grande | | | | | |  | |  |
|  |  | Campal Panaji Goa403001 | | | |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Sr. No** | **Image** | **Item Description** | **QTY** | **Price Per Unit** | **Total** |
| 1 |  | **Jacuzzi Massage Bath Tub** | 1 | 144067 | 144067 |
| Jacuzzi system with 6 hydrojets Body Jet big |
| Whirlpool Motor 1.5 HP |
| Fully Body Stand SS 316 |
| Pop Drainage System |
| Bubble bath with 24 jet Supported air blower |
| 12 Micro jets |
| Spinal Massager Jet 12 PCS 4 foot massager 8 back massager |
| Bubble blower 0.5hp |
| Multicolor 2 Led light chromatography 7 colour change |
| Designer Headrest pillow 2 psc |
| Full Water Capacity |
| Jacuzzi ON/OFF push button speed controller regulator |
| Bubble ON/OFF push button |
| Fully computerized control panel |
| Filler set hot cold and mixture diverter spout hand shower 3 flow system |
| Touch screen with control panel |
| Water level controller |
| Stereo phonic radio FM |
| Bluetooth & aux music system |
| Automatic Shut |
| Earth leakage circuit breaker |
| Suction unit |
| Self draining pipes |
| Ozonizer |
| wooden frame |
| online heater |
| Size 6\*5\*2fit |
| 2 | **S S Steam Generator** | | 1 | 16949.1 | 16949 |
| SS outer body | |
| SS 316 Water tank | |
| Digital control panel operated | |
| Auto time cut off​ system | |
| Safety value brush | |
| Drain value brush | |
| Soil noise value | |
| Steam head | |
| Time and​ temperature control | |
| Digital control | |
| Auto temperature cut off system | |
| Auto draining​ system | |
| Stainless steel 304 grade 16 grade steam tank | |
| Stainless steel make heating element​ for long life | |
| 26mm thickness PUF insolution | |
| DRP for heating element | |
| Water level sensor​ cut off to ensure heater safety | |
| Safety pressure release value | |
| Flexible house connector for​ water fidding | |
| Steam diff user outlet | |
| Soft touch swithess | |
| LED display panel | |
| Stainless​ steel socket for long life | |
| Short circuit protection | |
| High current protection | |
| Earth leakage Steam generator 6kw | |
| **Total** | | | | | **161016** |
| **GST 18%** | | | | | **28983** |
| **Grand Total** | | | | | **189999** |

**Payment Terms**

50% Advance

Balance on Delivery

**Warranty Terms**

5 years warranty on motor

10 years warranty on tub

2 years warranty on rest

Terms and conditions apply as per norms JPT001

Prices are inclusive of freight, logistics, handling, taxes, etc complete with door delivery at the address mentioned as shipping address.

Kindly dispatch the material as per quotation mentioned

Payment after receipt of material

If required Installation Engineer / personal will have to come to the site and complete the process at no extra cost